\section{Cablecast 4.7.9 Release Notes}
\begin{description}

\item[{\color{red}
\textbf{3612} \textbf{JVCMV232CM does not implement RecordStop}
\textbf{The JVCMV232 Control Module now implements RecordStop.}
\item[{\color{red}
\textbf{3758} \textbf{Some Windows Media Encoder Profiles are Corrupt}
\textbf{All of the Profiles (.prx files) that VOD and live streaming use are now working correctly.}
\item[{\color{red}
\textbf{3763} \textbf{Live IP Video has duplicate areas to set Connection Limit}
\textbf{Live Streaming now only uses the setting in the WebUI. Changes to the connection limit require the setting to be saved, then streaming must be stopped and restarted.}
\item[{\color{red}
\textbf{3769} \textbf{VOD Servers will sometimes re-transcode the same file, even if it has sucessfully been transcoded before.}
\textbf{VOD servers will no longer attempt to re-transcode a file that already exists.}
\item[{\color{red}
\textbf{3771} \textbf{Live streaming does not always start and stop as it should}
\textbf{Live streaming servers will now start and stop as expected.}
\item[{\color{red}
\textbf{3773} \textbf{Sony DVP777CM give 'Object reference not set to an instance of an object' when attempting to get status}
\textbf{Resolved an issue that was preventing the control module from getting the status of the device.}
\item[{\color{red}
\textbf{3777} \textbf{VS4 reverts to composite from component after restart}
\textbf{It is now possible to set VS4 servers to output a YUV signal in the CablecastDeviceControl.exe.config file.}
\end{description}

