\section{Cablecast 4.8.7 Release Notes}
\begin{description}

\item[{\color{red}
\textbf{5280} \textbf{LiveIP Exempt creates Switch to 0 (zero)}
\textbf{When sending autopilot on systems STRM-LIVE servers, autopilot would add a switch command to input 0. On some system this caused routing switchers to take to unexpected inputs.}
\item[{\color{red}
\textbf{5328} \textbf{Knox64CM router status does not report consistently}
\textbf{Some Knox64 router do not report their status in a consistent way, we made Cablecast's processing code more robust to handle these inconsistencies.}
\end{description}

