\section{Cablecast 4.9.1 Release Notes}
\begin{description}

\item[{\color{red}
\textbf{4433} \textbf{Stopped automation does not affect bug/text}
\textbf{DSK information will now adhere to an overridden channel and not follow the original schedule.}
\item[{\color{red}
\textbf{5486} \textbf{Add ability to change Podcast content location}
\textbf{Podcasts can now have their storage location changed on the server. This requires changing system settings.}
\item[{\color{red}
\textbf{5487} \textbf{AutoPatchBCSCM supports router levels}
\textbf{Added the ability to define what levels of the router should be controlled via the AutoPatchBCSCM.}
\item[{\color{red}
\textbf{5551} \textbf{Reintroduce Standalone mode for Luminance Keyed DSK}
\textbf{Reintroduced the classic "Standalone" mode for CablecastDSK. This mode allows the use of luminance keying to display DSK information.}
\item[{\color{red}
\textbf{5554} \textbf{Drag and drop scheduling won't populate DSK fields}
\textbf{DSK fields within a scheduled show will now populate correctly from the source ShowID when you drag and drop it into the schedule.}
\item[{\color{red}
\textbf{5579} \textbf{ChyTV can become unresponsive to CablecastDSK}
\textbf{Resolved a situation where the ChyTV would become unresponsive after a large number of commands had been sent to it.}
\item[{\color{red}
\textbf{5607} \textbf{Panasonic ControlModules can stop responding}
\textbf{Resolved an issue where the Panasonic ControlModules could seize a serial port, causing the system to respond incorrectly for a period of time.}
\item[{\color{red}
\textbf{5623} \textbf{Kramer2000CM interfaces with Kramer SDI Routers}
\textbf{Kramer SDI routers with embedded audio will now correctly return status.}
\end{description}

