\section{Cablecast 5.0.8 Release Notes}
\begin{description}

\item[{\color{red}
\textbf{6956} \textbf{SX-Live servers fail if using AT&T U-verse profile}
\textbf{SX-Live Servers can now make use of the AT&T profile. This may require updating the CablecastDeviceControl application configuration file on certain servers.}
\item[{\color{red}
\textbf{7130} \textbf{Device Assignments do not show 'Record' assignments}
\textbf{The Device Assignment listing now shows record devices.}
\item[{\color{red}
\textbf{7140} \textbf{Force Menu Breaks When Certain Characters Are Present In Output Name}
\textbf{Fixes an issue where certain characters such as ampersands would cause the Force Matrix not to work properly.}
\item[{\color{red}
\textbf{7342} \textbf{Cablecast does not create Play events for manual records where the source is a Digital File device}
\textbf{The correct play events are now created for record runs that have a digital file device as a source.}
\item[{\color{red}
\textbf{7421} \textbf{SX sometimes encodes faster than real time}
\textbf{Fixed an issue where a corrupt video signal could cause the SX to record faster than real time resulting in large and unusable files.}
\item[{\color{red}
\textbf{7481} \textbf{Cablecast fails to find files that were previously deleted}
\textbf{This fixes an issue where files that were removed from a video server's content drive and then added back at a later date would fail to be recognized. Cablecast will now find the files when they are re-added.}
\item[{\color{red}
\textbf{7487} \textbf{SXConfiguration  playback progress bar is not accurate}
\textbf{The playback progress bar now accurately represents the current position of the file being played.}
\item[{\color{red}
\textbf{7498} \textbf{Web Interface allows users to delete all of their Locations}
\textbf{Users can no longer delete all locations. Cablecast must have at least one location.}
\item[{\color{red}
\textbf{7534} \textbf{Cablecast Control Module guide is missing serial port diagrams}
\textbf{The images are now back where they belong.}
\item[{\color{red}
\textbf{7562} \textbf{UtahScientificRCP1CM does not work correctly with 100x series routers}
\textbf{Newer Utah 100x routers do not respond with a termination character required by the RCP-1 protocol We have removed the requirement for this character from the UtahRCP control module.}
\end{description}

