\section{Cablecast 5.4.0 Release Notes}
\begin{description}

\item[{\color{red}
\textbf{8296} \textbf{Cablecast is able to send GPI triggers}
\textbf{Manual Events can now be used to trigger GPI devices.}
\item[{\color{red}
\textbf{8358} \textbf{Genlock settings can be adjusted with SX Configuration application}
\textbf{Adjustments have been added for Horizontal and Vertical delay.}
\item[{\color{red}
\textbf{8384} \textbf{SX Servers are unable to play back or validate files recorded by Synergy servers}
\textbf{Resolved an issue that was preventing files recorded on Synergy equipment from playing back on SX servers.}
\item[{\color{red}
\textbf{8395} \textbf{SX Servers can be set for separate encode and decode resolutions}
\textbf{The SX Configuration application now allows the encode and decode resolutions to be set independently.}
\item[{\color{red}
\textbf{8414} \textbf{Allow LeitchRouterCM to control routers over IP}
\textbf{The LeitchRouterCM can now control routers over an IP or serial connection.}
\end{description}

