\section{Cablecast 5.4.2 Release Notes}
\begin{description}

\item[{\color{red}
\textbf{8445} \textbf{Support for the NV9000 router protocol}
\textbf{Added support for the NV9000 protocol via the NV9000CM. This allows support for Miranda routers that use the NV9000 protocol.}
\item[{\color{red}
\textbf{8513} \textbf{Improve SXConfiguration display of genlock timing adjustments}
\textbf{The vertical delay is now given in lines instead of nanoseconds which is more consistent with video test equipment.}
\item[{\color{red}
\textbf{8570} \textbf{Generation of MPEG-2 index files may timeout prematurely on SX servers}
\textbf{Increased the timeout for MPEG index generation to allow larger files to completely index.}
\item[{\color{red}
\textbf{8571} \textbf{Sigma routers can miss simultaneous switches}
\textbf{Resolved an issue that could cause a Sigma router to miss one or more switches when multiple events occurred at the same time.}
\end{description}

