\section{Carousel-for-BrightSign-Players 1.2.0 Release Notes}
\begin{description}

\item[{\color{red}
\textbf{8718} \textbf{Updated User Interface for the BrightSign Player Configuration Tool for Carousel }
\textbf{UI has been updated for Monitor Control with both RS-232 and Power Save.}
\item[{\color{red}
\textbf{8721} \textbf{BrightConfig App Renamed to BrightSign Player Configuration Tool for Carousel}
\textbf{The BrightConfig App has been renamed to the BrightSign Player Configuration Tool for Carousel for clarity of purpose and functionality.}
\item[{\color{red}
\textbf{8964} \textbf{RS-232 Monitor Control}
\textbf{RS-232 Monitor Control functionality has been added to the BrightSign Player Configuration Tool for Carousel, on the Monitor Control tab. Hexadecimal on/off commands and baud rate, as specified by the monitors manufacturer, are sent at the times specified in the Monitor Control tab.}
\item[{\color{red}
\textbf{9068} \textbf{Wireless Module Will Not Connect to Wireless Network}
\textbf{The Network Diagnostics Tool, that displays at player startup, no longer tests ethernet in a loop when the wireless module is enabled.}
\item[{\color{red}
\textbf{9112} \textbf{Power Save Monitor Control  }
\textbf{Power Save Monitor Control functionality has been added to the BrightSign Player  Configuration Tool for Carousel, on the Monitor Control tab. VGA/HDMI ports can be turned on and off at specified times.}
\end{description}

