\section{Cablecast 4.7.2 Release Notes}
\begin{description}

\item[{\color{red}
\textbf{2710} \textbf{SX servers abort records when video signal is lost}
\textbf{The SX encoder will now drop frames if its signal is interrupted.}
\item[{\color{red}
\textbf{2761} \textbf{SX playback has error with some files that need scaling}
\textbf{Resolved an issue that prevented the SX from playing some files that it is capable of playing.}
\item[{\color{red}
\textbf{2800} \textbf{SX Encoder CM does not support MoveFile}
\textbf{The SXEncoder Control module now supports Moving files after an encode has completed.}
\item[{\color{red}
\textbf{2803} \textbf{SX Player application crashes when playing unsupported video}
\textbf{The SX Player handles unsupported video more gracefully.}
\item[{\color{red}
\textbf{2836} \textbf{Digital File Managemnt does not correctly calculate record time for SX}
\textbf{Digital File Management will now correctly calculate the time remaining on disk.}
\item[{\color{red}
\textbf{2838} \textbf{Crawls in the manual schedule can't be longer than 28 hours}
\textbf{Resolved an issue that was preventing the user from creating long manual crawls.}
\item[{\color{red}
\textbf{2839} \textbf{Autopilot creates a conflict when there should not be one}
\textbf{Resolved an issue that was causing problems with back-to-back playback from some devices.}
\item[{\color{red}
\textbf{2844} \textbf{Link Electronics AVS-816CM}
\textbf{the LinkAVSCM is now available for routing switcher control.}
\item[{\color{red}
\textbf{2854} \textbf{DSK support for Compix G3 hardware}
\textbf{DSK now supports the new generation of hardware from Compix.}
\item[{\color{red}
\textbf{2856} \textbf{SX Playback skips several frames when a record stops}
\textbf{The SX will no longer drop frames on playback when a record stops.}
\item[{\color{red}
\textbf{2868} \textbf{SX occasionally delays playback by 2-3 seconds}
\textbf{Under certain circumstances, the SX would play shows 2-3 seconds late.  This has been resolved.}
\end{description}

