\section{Cablecast 5.0.3 Release Notes}
\begin{description}

\item[{\color{red}
\textbf{5539} \textbf{Support for Select Blackmagic Design Video Hub routers}
\textbf{The Micro, Smart, and Compact Videohub routers are now supported using the LeitchRouter Control Module.}
\item[{\color{red}
\textbf{6367} \textbf{Encodes on SX servers with no file key specified are not named}
\textbf{When an encode has no file key we will now name the file based on the current date and time.}
\item[{\color{red}
\textbf{6382} \textbf{When adding a new run in the schedule cursor should default to ShowID}
\textbf{After a new run is placed in the schedule the cursor is placed in the ShowID field so a showID number can be typed.}
\item[{\color{red}
\textbf{6383} \textbf{Implement V-chip rating for Evertz 8084AD}
\textbf{The Evertz 8084AD can now be used to embed v-chip ratings  in a channels output.}
\item[{\color{red}
\textbf{6385} \textbf{h264 video longer than 45 minutes will stutter}
\textbf{Video files exported from Apple compressor longer than 45 minutes would stutter after the 45 minute mark. These files now playback properly.}
\item[{\color{red}
\textbf{6386} \textbf{Timecode VTR devices do not cue properly}
\textbf{Timecode VTR devices now will now properly handle a cue command.}
\item[{\color{red}
\textbf{6387} \textbf{Cue and Play Events for RecordSourceEvents are incorrect}
\textbf{Cue and play event times for sources of record events were are now correctly timed.}
\item[{\color{red}
\textbf{6389} \textbf{SX Servers have playback issues due to aggressively indexing new files}
\textbf{SX Servers now wait until a file is done being written before attempting to index the file.}
\item[{\color{red}
\textbf{6403} \textbf{Improve Fill Gaps with Project Batch Function}
\textbf{Fill gaps batch function will not schedule the same show multiple times in a gap unless the Allow Repeats option is selected.}
\item[{\color{red}
\textbf{6409} \textbf{Disabled or Deleted devices can cause Autopilot to error out}
\textbf{Deleted or Disabled devices can cause Autopilot sends to error out.}
\item[{\color{red}
\textbf{6411} \textbf{Not all outputs on SX4 respect external genlock setting}
\textbf{When changing the Genlock source in SXConfiguration the setting will propagate to all outputs.}
\item[{\color{red}
\textbf{6417} \textbf{SX encoder sometimes encodes faster than real time}
\textbf{On rare instances improperly timestamped video frames would cause the SX encoder to record a single frame faster than real time. These bad frames will now be discarded and the endcode will continue normally.}
\item[{\color{red}
\textbf{6424} \textbf{Add SQL Server 2005 as an installer requirement}
\textbf{Cablecast installer now checks for SQL Server 2005 before continuing with installation.}
\item[{\color{red}
\textbf{6429} \textbf{Add ftp digital file managment to VDCPCM}
\textbf{VDCPCM will now poll for digital files using FTP if an IP address is entered into the Network Path CM setting.}
\end{description}

