\section{Cablecast 6.0.0 Release Notes}
\begin{description}

\item[{\color{red}
\textbf{941} \textbf{System Time is shown in Cablecast Menu Bar}
\textbf{The server's current time is now shown in the Cablecast Menu Bar.}
\item[{\color{red}
\textbf{3146} \textbf{Enhanced Blocking}
\textbf{The new Advanced Paste functionality includes support for blocks that are greater than one week long as well as other improvements.}
\item[{\color{red}
\textbf{3309} \textbf{Redesign Main Menu as a system dashboard}
\textbf{The Cablecast Main Menu now provides many more details about the systems' operational state.}
\item[{\color{red}
\textbf{6454} \textbf{Schedule includes Undo and Redo}
\textbf{The Schedule now includes Undo and Redo functionality.}
\item[{\color{red}
\textbf{6582} \textbf{Redesigned Public Site}
\textbf{Created a completely new Public Site that includes much better Live Streaming, Video on Demand and search functionality with enhanced customization options.}
\item[{\color{red}
\textbf{7799} \textbf{Redesigned Menu navigation pages}
\textbf{Redesigned menu pages to include help text for each item in addition to other improvements.}
\item[{\color{red}
\textbf{7978} \textbf{Redesigned Schedule}
\textbf{The Scheduling interface has been completely redesigned for better performance and more intuitive operation.}
\item[{\color{red}
\textbf{8427} \textbf{SX servers support 25 and 50 fps input and output resolutions}
\textbf{The SX servers can now be set to output PAL frame rate resolutions such as 720p at 50 frames per second.}
\item[{\color{red}
\textbf{8428} \textbf{SX Servers Support 1080p / 3G-SDI / SMPTE 425 Level A}
\textbf{SX HD video servers now support 1080p as an encode and decode resolution.}
\item[{\color{red}
\textbf{8499} \textbf{Servers page displays time delta between machines}
\textbf{The System Settings : Servers page now includes the time difference between machines.}
\item[{\color{red}
\textbf{8514} \textbf{Control Modules log the executed time of an event}
\textbf{The Cablecast Control Modules now log the exact time at which they executed an event in addition to the time at which it was scheduled.}
\item[{\color{red}
\textbf{8515} \textbf{Servers page displays TeamViewer ID}
\textbf{The System Settings : Servers page now includes the TeamViewer ID number for each configured server.}
\item[{\color{red}
\textbf{8536} \textbf{Interstitial should default to zero seconds}
\textbf{The default interstitial length is now zero instead of 45 seconds.}
\item[{\color{red}
\textbf{8543} \textbf{SX servers support mixed frame rates}
\textbf{SX video servers can now play files with different frame rates without changing the server's output resolution as long as the files frame rate is in the same family as the server's output resolution.}
\item[{\color{red}
\textbf{8757} \textbf{SX servers show time remaining in Force Menu}
\textbf{The time remaining for the current file is now shown in the Cablecast Force Menu.}
\item[{\color{red}
\textbf{8829} \textbf{Cablecast RESTful API}
\textbf{An all-new RESTful JSON & XML API is now available.}
\item[{\color{red}
\textbf{8833} \textbf{Redesigned Show Search pages}
\textbf{The Show Search functions have been completely redesigned.}
\item[{\color{red}
\textbf{8858} \textbf{Completely new Cablecast User Guide}
\textbf{Wrote a completely new Cablecast user guide with a focus on providing a easy to use reference guide.}
\item[{\color{red}
\textbf{8861} \textbf{Redesigned Show screen}
\textbf{The Show screen has been redesigned to be more efficient on mobile devices in addition to many other improvements.}
\item[{\color{red}
\textbf{9020} \textbf{Cablecast Service creates scaled down thumbnails of digital files}
\textbf{The Cablecast Service now creates scaled versions of thumbnails, so they can be used more effectively.}
\end{description}

