\section{Carousel-for-BrightSign-Players 1.3.0 Release Notes}
\begin{description}

\item[{\color{red}
\textbf{8970} \textbf{BrightSign Diagnostic Web Server can be Enabled From the BrightSign Player Configuration Tool for Carousel}
\textbf{The Diagnostic Web Server (DWS) is accessed in the Advanced Tab of the BrightSign Player Configuration Tool for Carousel. Please note, the only way to disable the DWS is by using the Reset Tool (see 9327).}
\item[{\color{red}
\textbf{9154} \textbf{Player Does Not Update When Cache Fills SD Card}
\textbf{Content stored on the SD card is now deleted if it's no longer in use.}
\item[{\color{red}
\textbf{9211} \textbf{Launching a Full Screen Alert Video Bulletin While a Zone is Playing a Video Locks Display}
\textbf{Full Screen Alert Videos now play as expected when a video is playing in a zone.}
\item[{\color{red}
\textbf{9229} \textbf{Players Freezing and Requiring Restart}
\textbf{Corrupt content no longer causes players to freeze.}
\item[{\color{red}
\textbf{9321} \textbf{Reimplementation of CEC Monitor Control Over HDMI}
\textbf{CEC Monitor Control has been reimplemented. Default on/off commands are sent to supported displays via HDMI.}
\item[{\color{red}
\textbf{9327} \textbf{Player Reset Tool}
\textbf{The Player Reset Tool is located in the Advanced Tab of the BrightSign Player Configuration Tool for Carousel. It provides a single script to use with an SD card to reset your BrightSign player to factory settings.}
\item[{\color{red}
\textbf{9328} \textbf{Serial Logging Toggle}
\textbf{The serial logging toggle is found in the Advanced Tab of the BrightSign Player Configuration Tool for Carousel.}
\item[{\color{red}
\textbf{9458} \textbf{Streaming Video Alert Bulletins Freeze When Stream Cannot be Found at the Time the Bulletins is Scheduled to Play}
\textbf{Players will now wait for the stream to return and will display once it's available.}
\item[{\color{red}
\textbf{9493} \textbf{Server Installer Removes Former Firmware Files}
\textbf{Previous firmware files are removed prior to installing the latest version of firmware.}
\item[{\color{red}
\textbf{9506} \textbf{International Time Zone Support}
\textbf{International time zones are selected in the BrightSign Player Configuration Tool for Carousel.}
\item[{\color{red}
\textbf{9693} \textbf{Non-fully Qualified Domains do Not Resolve}
\textbf{Set up in the BrightSign Player Configuration Tool for Carousel requires, Fully Qualified Domain Names. Help text, 'Enter the IP address or FQDN' was added to the Tightrope Server IP Address field.}
\end{description}

